|  |  |
| --- | --- |
| **Component** | **Label** |
| Capacitor | C |
| Resistor | R |
| Inductor | H |
| Diode | D |
| LED | L |
| IC | I |

To label components:

* Open ImageLabeler
* Load “Label Definitions” ([see this file](https://drive.google.com/open?id=1sPhxzYTwEi7u6XMjvOxnXtkX4V5fYjTa) in the current folder, ‘valid\_labels.mat’)
* Annotate using these types
* Export ground truth to .mat file using “Export Labels” → “To File”
* [Optionally] save session